Product Specifications: SlimFit Union™ 
Overview
The SlimFit Union™ Benchmark Test Point is designed for use in ASD sampling pipe networks, providing reliable and efficient performance at the end of each pipe branch.
Specifications
•	Product Name: SlimFit Union™ Benchmark Test Point
•	Pipe Compatibility: Fits 3/4" pipe
o	Connection Options: Threaded connection or optional slip fit insertion
•	Operation:
o	Normally closed, fail-safe design
o	No external components required for operation
•	Testing Port:
o	Integral chamfered 1/8” port for easy access during testing
•	Integrated Technology:
o	Equipped with an NFC chip
o	Stores information including:
•	Unique serial number
•	Associated detector and location
•	Commissioning benchmark data
•	Subsequent inspection test data
o	Data protection: Permanently stored and safeguarded against unauthorized deletion
•	Label Material:
o	Constructed from durable PET material
•	Properties:
o	Antistatic
o	Waterproof
o	Chemical resistant
o	Self-peel resistant
•	Label Content:
o	Pre-printed with:
•	NFC identifier indicating NFC capability
•	Part number
•	QR code containing a unique serial number for the test point
Compatibility and Management
•	Data Retrieval:
o	NFC and QR code data retrieval and management compatible with:
•	iOS devices
•	Android devices
•	App Integration:
o	Designed for use with a compatible app intended for ASD commissioning, testing, and inspection.